//
// Description: WAV to AC3 Encoder Translation File
// Version: 5.4
// Charset: Unicode
// Translator: Wiesław Šoltés
//

//
// Translation Language Name: in English
//

0x00000001=English

//
// Translation Language Name: in target language
//

0x00000002=English

//
// Main Dialog: Main Menu
//

0x00101001=&File
0x00101002=Add &Files...\tCtrl+F
0x00101003=Add &Directory...\tCtrl+D
0x00101004=&MUX Wizard...\tCtrl+M
0x00101005=L&oad Files List...\tCtrl+O
0x00101006=Sa&ve Files List...\tCtrl+S
0x00101007=&Load Presets...\tCtrl+Shitf+O
0x00101008=&Save Presets...\tCtrl+Shitf+S
0x00101009=E&xit\tAlt+F4

0x00102001=&Options
0x00102002=Disable All &Warnings\tCtrl+Shift+W
0x00102003=Save Configuration On E&xit\tCtrl+Shift+C
0x00102004=Loa&d Configuration\tF7
0x00102005=Sav&e Configuration\tF8

0x00103001=&Language
0x00103002=&Default (English)

0x00104001=&Help
0x00104002=Command-&Line Help\tCtrl+F1
0x00104003=&Website\tCtrl+Shift+W
0x00104004=&About...\tCtrl+Shift+A

//
// Main Dialog: Buttons
//

0x00201001=&Encode
0x00201002=Rese&t
0x00201003=&Remove
0x00201004=A&dd
0x00201005=&Add files...
0x00201006=&...
0x00201007=MU&X Wizard...
0x00201008=Ed&it

//
// Main Dialog: Static Text
//

0x00202001=Preset:
0x00202002=Quality:
0x00202003=Bitrate:
0x00202004=Value:
0x00202005=Sample format:
0x00202006=Sample rate:
0x00202007=Channels:
0x00202008=Engine:
0x00202009=Threads:
0x0020200A=M&ultiple mono input
0x0020200B=Output file:
0x0020200C=Output path:

//
// Main Dialog: Files List
//

0x00203001=File path
0x00203002=File size (bytes)

//
// Main Dialog: Files List Context-Menu
//

0x00204001=&List
0x00204002=Add &Files...\tCtrl+F
0x00204003=Add &Directory...\tCtrl+D
0x00204004=&MUX Wizard...\tCtrl+M
0x00204005=L&oad Files List...\tCtrl+O
0x00204006=Sa&ve Files List...\tCtrl+S
0x00204007=Move &Up\tCtrl+Up
0x00204008=Move Dow&n\tCtrl+Down
0x00204009=Remove &Selected Files\tDel
0x0020400A=Remove &All Files\tCtrl+Del

//
// Main Dialog: Settings List
//

0x00205001=Option
0x00205002=Value

//
// Main Dialog: Tooltips
//

0x00206001=CBR bitrate in kbps:\n\nCBR mode is selected by default. This option allows for\nsetting the fixed bitrate. The default bitrate depends\non the number of channels (not including LFE).\n1 = 96 kbps\n2 = 192 kbps\n3 = 256 kbps\n4 = 384 kbps\n5 = 448 kbps\n\nVBR quality:\n\nA value 0 to 1023 which corresponds to SNR offset, where\nq=240 equates to an SNR offset of 0. 240 is the default\nvalue. This scale will most likely be replaced in the\nfuture with a better quality measurement.
0x00206002=Enable VBR mode. If unchecked the CBR mode is used instead.
0x00206003=Set currently used encoder preset. You can load/save presets from/to file\nfrom File menu. All presets are automatically loaded/saved from/to text file.
0x00206004=Aften will auto-detect available SIMD instruction sets\nfor your CPU, so you shouldn't need to disable sets\nexplicitly - unless for speed or debugging reasons.
0x00206005=This option enables MMX optimizations (if supported by CPU).\n\n
0x00206006=This option enables SSE optimizations (if supported by CPU).\n\n
0x00206007=This option enables SSE2 optimizations (if supported by CPU).\n\n
0x00206008=This option enables SSE3 optimizations (if supported by CPU).\n\n
0x00206009=Raw audio input sample format specifies the sample format\nwhen using raw audio input. Using this option forces Aften to\ntreat the input as raw audio. The choices for the\npre-defined sample formats are (default: s16_le):\nu8, s16_le, s16_be, s20_le, s20_be, s24_le, s24_be,\ns32_le, s32_be, float_le, float_be, double_le, double_be
0x0020600A=Raw audio input sample rate option forces Aften to\ntreat the input as raw audio (default: 48000).
0x0020600B=Raw audio input channels forces Aften to treat the input as\nraw audio (default: 2).
0x0020600C=Aften can use multiple threads to speed up encoding.\nBy default, Aften uses one thread for each logical CPU\nyour system has, but you can override this value. A\nvalue of 0 is the default and indicates that Aften\nshould try to detect the number of CPUs.
0x0020600D=Set currently used Aften library. By selecting optimized Aften\nlibrary you can speedup the encoding process.
0x0020600E=Set default output path for encoded files. By default files\nare encoded to the same directory as input files. When using\nmultiple mono input than here is set the output file path.
0x0020600F=Enable multiple mono input mode. By adding multiple mono input\nfiles to the files list (minimum 2, maximum 6) in correct channel\norder the mono input files will be encoded into single ac3 file.
0x00206010=Edit currently available Aften engines.

//
// Main Dialog: Misc.
//

0x00207001=Default
0x00207002=<Auto>
0x00207003=<Ignored>
0x00207004=<Same as input file path>
0x00207005=<Same as first input file path + output.ac3>
0x00207006=Supported Files
0x00207007=Files
0x00207008=All Files
0x00207009=Failed to allocate memory for filenames buffer!
0x0020700A=Fatal Error
0x0020700B=Add directory with supported input files:
0x0020700C=Remove all files from list and add files selected in MUX Wizard?\n\nNote: The channel configuration for current preset will be adjusted.
0x0020700D=MUX Wizard
0x0020700E=Supported Files (*.files;*.mux)|*.files;*.mux|Files List (*.files)|*.files|MUX Files (*.mux)|*.mux|All Files (*.*)|*.*||
0x0020700F=Preconfigured Presets (*.presets)|*.presets|All Files (*.*)|*.*||
0x00207010=Error
0x00207011=Add at least one file to the file list!
0x00207012=Supported are minimum 1 and maximum 6 mono input files!
0x00207013=Failed to load libaften.dll dynamic library!
0x00207014=Disable 'Multiple mono input' mode in order to use Avisynth scripts!
0x00207015=Invalid output path!
0x00207016=Invalid output file!
0x00207017=Failed to create output path!
0x00207018=Encoded %d mono files in %s (%0.3lf sec)
0x00207019=Encoded %d file%s in %s (%0.3lf sec)
0x0020701A=s
0x0020701B=New preset
0x0020701C=AC3 Files (*.ac3)|*.ac3|All Files (*.*)|*.*||
0x0020701D=Select default output path:
0x0020701E=Failed to load
0x0020701F=library
0x00207020=Loaded
0x00207021=version
0x00207022=Failed to initialize Avisynth
0x00207023=Sample format
0x00207024=unknown
0x00207025=Sample rate
0x00207026=Channels
0x00207027=Audio samples
0x00207028=Decoded size
0x00207029=AVS File Properties
0x0020702A=Error while searching for files!

//
// Main Dialog: Advanced Encoder Options Groups
//

0x00208001=Encoding options
0x00208002=Bitstream info metadata
0x00208003=Dynamic range compression and dialog normalization
0x00208004=Input options
0x00208005=Input filters
0x00208006=Alternate bit stream syntax

//
// Main Dialog: (1) Encoding options
//

0x00301001=Fast bit allocation
0x00301002=Fast bit allocation is a less-accurate search method\nfor CBR bit allocation. It only narrows down the SNR\nvalue to within 16 of the optimal value. The result\nis lower overall quality, but faster encoding. This\nmay not give the same results each time when using\nparallel encoding.
0x00301003=More accurate encoding (default)
0x00301004=Faster encoding

0x00302001=Exponent strategy search size
0x00302002=The encoder determines the best combination of\nexponent strategies for a frame by searching through\na list of pre-defined exponent strategies. This option\ncontrols the size of the list to be searched. The\nvalue can range from 1 (lower quality but faster) to\n32 (higher quality but slower). The default value is 8.
0x00302003=1 (lower quality but faster)
0x00302004=8 (default)
0x00302005=32 (higher quality but slower)

0x00303001=Start-of-stream padding
0x00303002=The AC-3 format uses an overlap/add cycle for encoding\neach block. By default, Aften pads the delay buffer\nwith a block of silence to avoid inaccurate encoding\nof the first frame of audio. If this behavior is not\nwanted, it can be disabled. The pad value can be a\n1 (default) to use padding or 0 to not use padding.
0x00303003=No padding
0x00303004=256 samples of padding (default)

0x00304001=Bandwidth
0x00304002=The bandwidth setting corresponds to the high-frequency\ncutoff. Specifically, it sets the highest frequency bin\nwhich is encoded. The AC-3 format uses a 512-point MDCT\nwhich gives 256 frequency levels from 0 to 1/2 of the\nsamplerate. The formula to give the number of coded\nfrequency bins from bandwidth setting is:\n(w * 3) + 73, which gives a range of 73 to 253\nThere are 2 special values, -1 and -2.\nWhen -1 is used, Aften automatically selects what\nit thinks is an appropriate bandwidth. This is the\ndefault setting.\nWhen -2 is used, a bandwidth is chosen for each frame\nbased on CBR frame size and a target quality of 240.\nVariable bandwidth cannot be used with VBR mode.
0x00304003=Fixed adaptive bandwidth (default)
0x00304004=Variable adaptive bandwidth
0x00304005=0 (28% of full bandwidth)
0x00304006=60 (99% of full bandwidth)

0x00305001=Minimum bandwidth
0x00305002=For variable bandwidth mode (-2), this option sets the\nminimum value for the bandwidth code. This allows the\nuser to avoid a harsh cutoff frequency by sacrificing\ngeneral audio quality. The default value is 0.
0x00305003=0 (default)

0x00306001=Maximum bandwidth
0x00306002=For variable bandwidth mode (-2), this option sets the\nmaximum value for the bandwidth code. This can be used\nto speed up encoding by using a lower value than 60,\nwhich is the default.
0x00306003=60 (default)

0x00307001=Stereo rematrixing
0x00307002=Using stereo rematrixing can increase quality by\nremoving redundant information between the left and\nright channels. This technique is common in audio\nencoding, and is sometimes called mid/side encoding.\nWhen this setting is turned on, Aften adaptively turns\nrematrixing on or off for each of 4 frequency bands for\neach block. When this setting is turned off,\nrematrixing is not used for any blocks. The default\nvalue is 1.
0x00307003=Independent L+R channels
0x00307004=Mid/side rematrixing (default)

0x00308001=Block switching
0x00308002=The AC-3 format allows for 2 different types of MDCT\ntransformations to translate from time-domain to\nfrequency-domain. The default is a 512-point transform,\nwhich gives better frequency resolution. There is also\na 256-point transform, which gives better time\nresolution. The specification gives a suggested method\nfor determining when to use the 256-point transform.\nWhen block switching is turned on, Aften uses the spec\nmethod for selecting the 256-point MDCT. When it is\nturned off, only the 512-point MDCT is used, which is\nfaster. Block switching is turned off by default.
0x00308003=Use only 512-point MDCT (default)
0x00308004=Selectively use 256-point MDCT

//
// Main Dialog: (2) Bitstream info metadata
//

0x00401001=Center mix level
0x00401002=When three front channels are in use, this code\nindicates the nominal down mix level of the center\nchannel with respect to the left and right channels.\n0 = -3.0 dB (default)\n1 = -4.5 dB\n2 = -6.0 dB
0x00401003=-3.0 dB (default)

0x00402001=Surround mix level
0x00402002=If surround channels are in use, this code indicates\nthe nominal down mix level of the surround channels.\n0 = -3 dB (default)\n1 = -6 dB\n2 = 0
0x00402003=-3 dB (default)

0x00403001=Dolby Surround mode
0x00403002=When operating in the two channel mode, this code\nindicates whether or not the program has been encoded in\nDolby Surround. This information is not used by the\nAC-3 decoder, but may be used by other portions of the\naudio reproduction equipment.\n0 = not indicated (default)\n1 = not Dolby surround encoded\n2 = Dolby surround encoded
0x00403003=Not indicated (default)
0x00403004=Not Dolby surround encoded
0x00403005=Dolby surround encoded

//
// Main Dialog: (3) Dynamic range compression and dialog normalization
//

0x00501001=Dialog normalization
0x00501002=The dialog normalization value sets the average dialog\nlevel. The value is typically constant for a particular\naudio program. The decoder has a target output dialog\nlevel of -31dB, so if the dialog level is specified as\nbeing -31dB already (default), the output volume is not\naltered. Otherwise, the overall output volume is\ndecreased so that the dialog level is adjusted down to\n-31dB.
0x00501003=31 (default)

0x00502001=Dynamic Range Compression profile
0x00502002=Dynamic Range Compression allows for the final output\ndynamic range to be limited without sacrificing quality.\nThe full dynamic range audio is still encoded, but a\ncode is given for each block which tells the decoder to\nadjust the output volume for that block. The encoder\nmust analyze the input audio to determine the best way\nto compress the dynamic range based on the loudness and\ntype of input (film, music, speech).\n0 = Film Light\n1 = Film Standard\n2 = Music Light\n3 = Music Standard\n4 = Speech\n5 = None (default)
0x00502003=Film Light
0x00502004=Film Standard
0x00502005=Music Light
0x00502006=Music Standard
0x00502007=Speech
0x00502008=None (default)

//
// Main Dialog: (4) Input options
//

0x00601001=Audio coding mode (overrides wav header)
0x00601002=The acmod and lfe options allow the user to explicitly select the\ndesired channel layout. This only controls the interpretation\nof the input, so no downmixing or upmixing is done.\n 0 = 1+1 (Ch1,Ch2)\n1 = 1/0 (C)\n2 = 2/0 (L,R)\n3 = 3/0 (L,R,C)\n4 = 2/1 (L,R,S)\n5 = 3/1 (L,R,C,S)\n6 = 2/2 (L,R,SL,SR)\n7 = 3/2 (L,R,C,SL,SR)

0x00602001=Specify use of LFE channel (overrides wav header)
0x00602002=The acmod and lfe options allow the user to explicitly select the\ndesired channel layout. This only controls the interpretation\nof the input, so no downmixing or upmixing is done.\n 0 = LFE channel is not present\n1 = LFE channel is present
0x00602003=LFE channel is not present
0x00602004=LFE channel is present

0x00603001=Specify channel configuration (overrides wav header)
0x00603002=The chconfig option allow the user to explicitly select the\ndesired channel layout. This only controls the interpretation\nof the input, so no downmixing or upmixing is done.\n 1+1 = (Ch1,Ch2)\n1/0 = (C)\n2/0 = (L,R)\n3/0 = (L,R,C)\n2/1 = (L,R,S)\n3/1 = (L,R,C,S)\n2/2 = (L,R,SL,SR)\n3/2 = (L,R,C,SL,SR)\nAdding +LFE indicates use of the LFE channel

0x00604001=Channel mapping order of input audio
0x00604002=Some programs create WAVE files which use a channel\nmapping other than the standard WAVE mapping. This\noption allows the user to specify if the input file\nuses WAVE, AC-3, or MPEG channel mapping. The MPEG\nchannel mapping is used by DTS and by MPEG-2/4 formats\nsuch as MP2 and AAC.\n0 = WAVE mapping (default)\n1 = AC-3 mapping\n2 = MPEG mapping
0x00604003=WAV mapping (default)
0x00604004=AC-3 mapping
0x00604005=MPEG mapping

0x00605001=Read input WAVE audio data until the end-of-file
0x00605002=This overrides the data size in the WAVE header, and\ncan be useful for streaming input or files larger than\n4 GB.\n0 = use data size in header (default)\n1 = read data until end-of-file
0x00605003=Use data size in header (default)
0x00605004=Read data until end-of-file

//
// Main Dialog: (5) Input filters
//

0x00701001=Specify use of the bandwidth low-pass filter
0x00701002=The bandwidth low-pass filter pre-filters the input\naudio before converting to frequency-domain. This\nsmooths the cutoff frequency transition for slightly\nbetter quality.\n0 = do not apply filter (default)\n1 = apply filter
0x00701003=Do not apply filter (default)
0x00701004=Apply filter

0x00702001=Specify use of the DC high-pass filter
0x00702002=The DC high-pass filter is listed as optional by the\nAC-3 specification. The implementation, as suggested,\nis a single pole filter at 3 Hz.\n0 = do not apply filter (default)\n1 = apply filter
0x00702003=Do not apply filter (default)
0x00702004=Apply filter

0x00703001=Specify use of the LFE low-pass filter
0x00703002=The LFE low-pass filter is recommended by the AC-3\nspecification. The cutoff is 120 Hz. The specification\nrecommends an 8th order elliptic filter, but instead,\nAften uses a Butterworth 2nd order cascaded direct\nform II filter.\n0 = do not apply filter (default)\n1 = apply filter
0x00703003=Do not apply filter (default)
0x00703004=Apply filter

//
// Main Dialog: (6) Alternate bit stream syntax
//

0x00801001=Specify use of extended bitstream info 1
0x00801002=Extended bitstream info 1 contains the dmixmod,\nltrtcmix, ltrtsmix, lorocmix, and lorosmix fields. If\nthis option is turned on, all these values are written\nto the output stream.\n0 = do not write xbsi1\n1 = write xbsi1
0x00801003=Do not write xbsi1
0x00801004=Write xbsi1

0x00802001=Preferred stereo downmix mode
0x00802002=This code indicates the type of stereo downmix preferred\nby the mastering engineer, and can be optionally used,\noverridden, or ignored by the decoder.\n0 = not indicated (default)\n1 = Lt/Rt downmix preferred\n2 = Lo/Ro downmix preferred
0x00802003=Not indicated (default)
0x00802004=Lt/Rt downmix preferred
0x00802005=Lo/Ro downmix preferred

0x00803001=Lt/Rt center mix level
0x00803002=This code indicates the nominal down mix level of the\ncenter channel with respect to the left and right\nchannels in an Lt/Rt downmix.\n0 = +3.0 dB\n1 = +1.5 dB\n2 =  0.0 dB\n3 = -1.5 dB\n4 = -3.0 dB (default)\n5 = -4.5 dB\n6 = -6.0 dB\n7 = -inf dB
0x00803003=-3.0 dB (default)

0x00804001=Lt/Rt surround mix level
0x00804002=This code indicates the nominal down mix level of the\nsurround channels with respect to the left and right\nchannels in an Lt/Rt downmix.\n0 = +3.0 dB\n1 = +1.5 dB\n2 =  0.0 dB\n3 = -1.5 dB\n4 = -3.0 dB (default)\n5 = -4.5 dB\n6 = -6.0 dB\n7 = -inf dB
0x00804003=-3.0 dB (default)

0x00805001=Lo/Ro center mix level
0x00805002=This code indicates the nominal down mix level of the\ncenter channel with respect to the left and right\nchannels in an Lo/Ro downmix.\n0 = +3.0 dB\n1 = +1.5 dB\n2 =  0.0 dB\n3 = -1.5 dB\n4 = -3.0 dB (default)\n5 = -4.5 dB\n6 = -6.0 dB\n7 = -inf dB
0x00805003=-3.0 dB (default)

0x00806001=Lo/Ro surround mix level
0x00806002=This code indicates the nominal down mix level of the\nsurround channels with respect to the left and right\nchannels in an Lo/Ro downmix.\n0 = +3.0 dB\n1 = +1.5 dB\n2 =  0.0 dB\n3 = -1.5 dB\n4 = -3.0 dB (default)\n5 = -4.5 dB\n6 = -6.0 dB\n7 = -inf dB
0x00806003=-3.0 dB (default)

0x00807001=Specify use of extended bitstream info 2
0x00807002=Extended bitstream info 2 contains the dsurexmod,\ndheadphon, and adconvtyp fields. If this option is\nturned on, all these values are written to the output\nstream. These options are not used by the AC-3 decoder,\nbut may be used by other portions of the audio\nreproduction equipment.\n0 = do not write xbsi2\n1 = write xbsi2
0x00807003=Do not write xbsi2
0x00807004=Write xbsi2

0x00808001=Dolby Surround EX mode
0x00808002=This code indicates whether or not the program has been\nencoded in Dolby Surround EX.\n0 = not indicated (default)\n1 = Not Dolby Surround EX encoded\n2 = Dolby Surround EX encoded
0x00808003=Not indicated (default)
0x00808004=Not Dolby Surround EX encoded
0x00808005=Dolby Surround EX encoded

0x00809001=Dolby Headphone mode
0x00809002=This code indicates whether or not the program has been\nDolby Headphone-encoded.\n0 = not indicated (default)\n1 = Not Dolby Headphone encoded\n2 = Dolby Headphone encoded
0x00809003=Not indicated (default)
0x00809004=Not Dolby Headphone encoded
0x00809005=Dolby Headphone encoded

0x0080A001=A/D converter type
0x0080A002=This code indicates the type of A/D converter technology\nused to capture the PCM audio.\n0 = Standard (default)\n1 = HDCD
0x0080A003=Standard (default)
0x0080A004=HDCD

//
// About Dialog
//

0x00901001=&OK
0x00901002=About WAV to AC3 Encoder
0x00901003=This program is free software; you can redistribute it and/or modify it under the terms of the GNU General Public License as published by the Free Software Foundation; version 2 of the License.
0x00901004=Version

//
// Work Dialog
//

0x00A01001=Encoding...
0x00A01002=&Cancel
0x00A01003=From:
0x00A01004=To:
0x00A01005=Elapsed time:
0x00A01006=Total elapsed time:
0x00A01007=Encoding:
0x00A01008=I/O Reads:
0x00A01009=I/O Writes:
0x00A0100A=Fatal Error
0x00A0100B=Failed to create worker thread!
0x00A0100C=Encoding file %d of %d
0x00A0100D=Encoding %d mono files

//
// Work Dialog: Current Job Info
//

0x00A02001=?
0x00A02002=?-channel
0x00A02003=Unsigned
0x00A02004=Signed
0x00A02005=Floating-point
0x00A02006=[unsupported type]
0x00A02007=1.1-channel
0x00A02008=2.1-channel
0x00A02009=3.1-channel
0x00A0200A=4.1-channel
0x00A0200B=5.1-channel
0x00A0200C=multi-channel with LFE
0x00A0200D=mono
0x00A0200E=stereo
0x00A0200F=3-channel
0x00A02010=4-channel
0x00A02011=5-channel
0x00A02012=6-channel
0x00A02013=multi-channel
0x00A02014=unknown
0x00A02015=little-endian
0x00A02016=big-endian
0x00A02017=Avisynth: Raw PCM Floating-point 32-bit little-endian
0x00A02018=dual mono (1+1)
0x00A02019=mono (1/0)
0x00A0201A=stereo (2/0)
0x00A0201B=NONE
0x00A0201C=Threads: Auto
0x00A0201D=Threads:

//
// Engines Dialog
//

0x00B01001=Engines Editor
0x00B01002=Engine
0x00B01003=Name:
0x00B01004=Path:
0x00B01005=&...
0x00B01006=&Import...
0x00B01007=&Export...
0x00B01008=&Add
0x00B01009=&Remove
0x00B0100A=&OK
0x00B0100B=&Cancel
0x00B0100C=Name
0x00B0100D=Path
0x00B0100E=DLL Files (*.dll)|*.dll|All Files (*.*)|*.*||
0x00B0100F=Aften Engines (*.engines)|*.engines|All Files (*.*)|*.*||

//
// MUX Dialog
//

0x00C01001=MUX Wizard
0x00C01002=Channel config:
0x00C01003=&Import MUX...
0x00C01004=&Export MUX...
0x00C01005=&OK
0x00C01006=&Cancel
0x00C01007=CLEAR
0x00C01008=Specify channel configuration:\n1+1 = (Ch1,Ch2)\n1/0 = (C)\n2/0 = (L,R)\n3/0 = (L,R,C)\n2/1 = (L,R,S)\n3/1 = (L,R,C,S)\n2/2 = (L,R,SL,SR)\n3/2 = (L,R,C,SL,SR)
0x00C01009=Indicates use of the LFE channel.
0x00C0100A=Front Left Channel
0x00C0100B=Front Right Channel
0x00C0100C=Front Center Channel
0x00C0100D=Low Frequency Effect Channel
0x00C0100E=Surround Left Channel
0x00C0100F=Surround Right Channel
0x00C01010=Surround Channel
0x00C01011=Supported Files (*.files;*.mux)|*.files;*.mux|Files List (*.files)|*.files|MUX Files (*.mux)|*.mux|All Files (*.*)|*.*||

//
// Command-Line
//

0x00D01001=WAV to AC3 Encoder Command-Line Help\n\nUsage: EncWAVtoAC3 [Options]\n\nOptions:\n\n-h, --help\nShow command-line help message.\n\n-x,--encode-and-exit\nEncode input files and exit.\n\n-r, --read-only\nDo not save configuration on exit.\n\n-i, --input-file <file.ext>\nSet input files path (*.wav, *.bin, *.pcm, *.raw, *.avs).\n\n-o, --output-file <file.ext>\nSet output file path (*.ac3).\n\n-d, --output-path <path>\nSet default output path (default: input file path is used).\n\n-c, --load-config <file.ext>\nLoad program configation (*.config).\n\n-f, --load-files <file.ext>\nLoad list of files to encode (*.files, *.mux).\n\n-p, --load-presets <file.ext>\nLoad list of preconfigured presets (*.presets).\n\n-e, --load-engines <file.ext>\nLoad list of Aften engines (*.engines).\n\n-m, --mux-wizard\nShow standalone MUX Wizard window.\n
0x00D01002=WAV to AC3 Encoder Command-Line Help\n\nUsage: EncWAVtoAC3 [Options]\n\nOptions:\n\n-h, --help\nShow command-line help message.\n\n-x,--encode-and-exit\nEncode input files and exit.\n\n-r, --read-only\nDo not save configuration on exit.\n\n-i, --input-file <file.ext>\nSet input files path (*.wav, *.bin, *.pcm, *.raw).\n\n-o, --output-file <file.ext>\nSet output file path (*.ac3).\n\n-d, --output-path <path>\nSet default output path (default: input file path is used).\n\n-c, --load-config <file.ext>\nLoad program configation (*.config).\n\n-f, --load-files <file.ext>\nLoad list of files to encode (*.files, *.mux).\n\n-p, --load-presets <file.ext>\nLoad list of preconfigured presets (*.presets).\n\n-e, --load-engines <file.ext>\nLoad list of Aften engines (*.engines).\n\n-m, --mux-wizard\nShow standalone MUX Wizard window.\n
0x00D01003=Command-Line Help
0x00D01004=Error
0x00D01005=Use --help option to obtain more informations.
0x00D01006=Invalid command-line argument!
0x00D01007=Unknown option Id!
0x00D01008=Input file is missing! Please use also --input-file option!.
0x00D01009=Can not combine --input-file with --load-files option!
0x00D0100A=Can not combine --output-file with --load-files option!
0x00D0100B=Can not combine --output-file with --output-path option!
