| Mixing RoomMachine 844 has an output mixer where the original dry signal is mixed with the wet signal taken from the virtual microphones. The gain of the original signal can be controlled with the DRY knob, while the amount of wet signal can be controlled with the WET knob. Alternatively, the balance between dry and wet can also be controlled by adjusting the distance between microphones and speakers and varying the wall damping accordingly. However, if it is crucial that the output contains undelayed dry signal, then the output mixer should be used. |
| © Copyright 2000, Hans Stadtherr. All rights reserved. Legal Notices, About