| Specifications
Plug-in type: | acoustic room simulation
Plug-in technology: | Steinberg VST
Operating system: | Microsoft Windows 95/98/NT
Compatible hosts: | all VST hosts, tested with Steinberg Cubase VST and Steinberg Wavelab
Memory requirement: | depends on samplerate, min. 1.4 Mbyte at 44.1 kHz, approx. 2.2 Mbyte at 96 kHz
Graphics adapter requirement: | High Color (16 bpp) recommended
Samplerate: | depends on VST host program, > 11 kHz recommended, no upper limit
Size of simulated room: | 3...150 meter length, 2...100 meter width
Audio precision: | 32 bit floatingpoint
Audio processing elements: | 8 delay lines, 8 lowpass filter, 44 delaying router
Filter type: | Butterworth, 6 dB / octave
Control parameters: | 10 (left pan, right pan, distance, stereowidth, roomsize, decay, wall damping, filter color, dry gain, wet gain)
Audio programs: | can be saved and loaded, 16 per bank, 10 editable factory programs
VST PlugIn Technology by Steinberg
| © Copyright 2000, Hans Stadtherr. All rights reserved. Legal Notices, About |